To check for issues in the digitalin file, read in the file

* digital\_data = readIntanDigitalFile(fname, varargin)
  + fname = ‘digitalin.dat’
  + plot the data
    - plot(digital\_data); % to plot the entire digitalin file
    - plot(digital\_data(1:200)); % to plot only a portion of the file (1:200), edit as needed.